**405nm PM Dual Stage Circulator (TGG Type)**

Ascentta expands its product line with several new additions in time for Laser World of Photonics Munich 2019!

**405nm Polarization Maintaining Dual Stage Circulator (TGG Type)**

PMS405XP Fiber

Isolation (23℃, All SOP) (2→1, or 3→2) Typ. 23dB, Min 20dB

Package Size Φ15 x L55mm

Optical Power Handling 30mW

Visit us at Laser World of Photonics Munich June 24th to June 27th 2019 at Booth: B2.B2.125!

For more information please visit us at Ascentta.com or email us at [sales@ascentta.com](mailto:sales@ascentta.com)

